**Control:**

It takes input from localization and planning to drive the steering wheel, acceleration and brake.

PID control( from control systems) algorithm is used to drive the controls because it is simple and powerful but it also has it’s cons.

So better alternatives are Linear Quadratic Regulator(LQR) and Model Predictive Control(MPC) algorithms.